Specification for beehives and other beekeeping equipment’s

1. **The modern hives** should be standard langstrom especially German type or standard Zander hives. Based on ES-2005. Frame should be flexible and fits to all boxes made of all seasoned standard wood with perfect measurements and nonrusting frame wire
2. The transitional hives should be from all seasoned dry wood and perfect measurement as stipulated on ES-2005. Ethiopian standard 2005, attached
3. Honey extractor four or three frame, stainless steel with strong top gear should be imported
4. Protective cloths (overall free size, veil and hand gloves free size, boots above 40 and mix of all size with more possible larger size)
5. Smokers = large size and from noon rusting strong stainless teel
6. Honey Presser = Imported and stainless steel and press more than 5kg at once
7. Wax stamper or casting molder =stainless eel or noon rusting, should be imported
8. Chisel = strong iron with yellow painted anti rust and imported
9. Fork or honey decamping fork =imported and standard for beekeeping
10. Queen excluder= Plastic and ES.2005 standard
11. Queen cage = plastic type
12. Honey strainer or double sieve = Stainless wire mesh, top part smaller hole and second part a bit larger hole size as the beekeeping standard